IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2016-06-09T16:49:08"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20140223_1515(x64) - Exporter 15.6.0.0 - Alternate UI 15.6.0.0"
Application: "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)"

People and organizations
  Person "Carlos" "M" of Organization (no name given)
  Owner history of Person "Carlos" "M" of Organization (no name given) | application "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Nombre de proyecto" | phase "Estado de proyecto"
  IFCSITE "Default" | latitude 40° 23′ 59.999999″ | longitude -3° 40′ 59.879999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Introduzca dirección aquí", "Madrid", "España"
      IFCBUILDINGSTOREY "Nivel 1" | long name "Nivel 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Eurocondens SGB 215" | object type "Eurocondens SGB 215" | names: "2014_2-Calderas_Baxi_de-Gas-de-Condensación-Eurocondens-SGB-125-300-en-cascada:Eurocondens SGB 215:132471" | material: materials ("Aleación aluminio-silicio acabado pintura - Baxi", "Cristal Display - Baxi", "Display - Baxi") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Cantidades de equipos mecánicos, Constraints, Dimensions, Identity Data

Types
  IFCBUILDINGELEMENTPROXYTYPE "Eurocondens SGB 215" | 1 occurrence | material: materials ("Aleación aluminio-silicio acabado pintura - Baxi", "Cristal Display - Baxi", "Display - Baxi") | property sets: Data, Dimensions, Identity Data, Materials and Finishes, Mechanical, Other

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Propietario" (IFCTEXT)
    Project Address = "Introduzca dirección aquí" (IFCTEXT)
    Project Issue Date = "Fecha de emisión" (IFCTEXT)
    Project Name = "Nombre de proyecto" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Estado de proyecto" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "2014_2-Calderas_Baxi_de-Gas-de-Condensación-Eurocondens-SGB-125-300-en-cascada: Eurocondens SGB 215" (IFCLABEL)
    Family and Type = "2014_2-Calderas_Baxi_de-Gas-de-Condensación-Eurocondens-SGB-125-300-en-cascada: Eurocondens SGB 215" (IFCLABEL)
    Separación Calderas Control = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "2014_2-Calderas_Baxi_de-Gas-de-Condensación-Eurocondens-SGB-125-300-en-cascada: Eurocondens SGB 215" (IFCLABEL)
    Type Id = "2014_2-Calderas_Baxi_de-Gas-de-Condensación-Eurocondens-SGB-125-300-en-cascada: Eurocondens SGB 215" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Extremo inicial 8 mm" (IFCLABEL)
    Family and Type = "Level: Extremo inicial 8 mm" (IFCLABEL)
    Type = "Level: Extremo inicial 8 mm" (IFCLABEL)
    Type Id = "Level: Extremo inicial 8 mm" (IFCLABEL)
  Other | properties | on 1 type object
    Altura Conexiones = 1444. (IFCLENGTHMEASURE) [MILLI METRE]
    Altura Tubo F = 1444. (IFCLENGTHMEASURE) [MILLI METRE]
    B = 280. (IFCLENGTHMEASURE) [MILLI METRE]
    C = 351. (IFCLENGTHMEASURE) [MILLI METRE]
    Category = "Mechanical Equipment" (IFCLABEL)
    D-C = 865. (IFCLENGTHMEASURE) [MILLI METRE]
    Diametro Exterior Gas = 52. (IFCLENGTHMEASURE) [MILLI METRE]
    Diametro Exterior IC-RC = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    Diametro Exterior Válvula Seguridad = 45. (IFCLENGTHMEASURE) [MILLI METRE]
    E = 122. (IFCLENGTHMEASURE) [MILLI METRE]
    E-1 = 302. (IFCLENGTHMEASURE) [MILLI METRE]
    E-2 = 163. (IFCLENGTHMEASURE) [MILLI METRE]
    F Exterior = 220. (IFCLENGTHMEASURE) [MILLI METRE]
    Family Name = "2014_2-Calderas_Baxi_de-Gas-de-Condensación-Eurocondens-SGB-125-300-en-cascada" (IFCTEXT)
    G = 851. (IFCLENGTHMEASURE) [MILLI METRE]
    H = 365. (IFCLENGTHMEASURE) [MILLI METRE]
    I = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    K = 80. (IFCLENGTHMEASURE) [MILLI METRE]
    L = 450. (IFCLENGTHMEASURE) [MILLI METRE]
    M = 167. (IFCLENGTHMEASURE) [MILLI METRE]
    N = 320. (IFCLENGTHMEASURE) [MILLI METRE]
    SGB 125 = FALSE (IFCBOOLEAN)
    SGB 170 = FALSE (IFCBOOLEAN)
    SGB 215 = TRUE (IFCBOOLEAN)
    SGB 260 = FALSE (IFCBOOLEAN)
    SGB 300 = FALSE (IFCBOOLEAN)
    SGB 400 = FALSE (IFCBOOLEAN)
    SGB 470 = FALSE (IFCBOOLEAN)
    SGB 540 = FALSE (IFCBOOLEAN)
    SGB 610 = FALSE (IFCBOOLEAN)
    Situación Gas = 96. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Extremo inicial 8 mm" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Nivel 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Autor = "Bimetica Parametric Design Services S.L." (IFCTEXT)
    Bimetica = "http://www.bimetica.com" (IFCTEXT)
    Catálogo tarifa = "http://www.baxi.es/docs/sp_cataleg/CatSept16_EuroCondens_SGB_gas.pdf/" (IFCTEXT)
    CondicionesGeneralesDeContratacion = "" (IFCTEXT)
    Declaración de conformidad CE = "http://www.baxi.es/docs/sp_decla/Decla_CE_Eurocondens_SGB.pdf" (IFCTEXT)
    Description = "Calderas de fundición de 125 kW de potencia útil, para instalaciones de Calefacción por agua caliente hasta 6 bar. Posibilidad integral de conexión doble en cascada homologada como un único generador." (IFCTEXT)
    DuracionVidaUtil = "" (IFCTEXT)
    EmailContacto = "solutions@baxi.es" (IFCTEXT)
    FechaEmisionElementoBIM = "04/05/2016" (IFCTEXT)
    FechaInstalacion = "" (IFCTEXT)
    FechaVencimientoElementoBIM = "01/01/2017" (IFCTEXT)
    Folleto media potencia = "http://www.baxi.es/docs/sp_folleta/folleto_MediaPotencia2015.pdf" (IFCTEXT)
    Homologación = "http://www.baxi.es/docs/sp_homo/homo_eurocondensSGB.pdf" (IFCTEXT)
    Manual Instalador = "http://www.baxi.es/docs/sp_instruc/SGB125-300H.pdf" (IFCTEXT)
    Manual Usuario = "http://www.baxi.es/docs/sp_instruc/SGB125-300_H_BAXI.pdf" (IFCTEXT)
    Manufacturer = "Baxi Calefacción, S.L.U." (IFCTEXT)
    Model = "2 calderas Eurocondens SGB 215 en cascada" (IFCTEXT)
    NumeroSerie = "Eurocondens SGB" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    PeriodoGarantia = "" (IFCTEXT)
    Referencia = "2 calderas Eurocondens SGB 215 en cascada" (IFCTEXT)
    ReferenciaContacto = "Departamento Técnico" (IFCTEXT)
    TelefonoContacto = "902 89 89 89" (IFCTEXT)
    Type Name = "Eurocondens SGB 215" (IFCTEXT)
    URL = "www.baxi.es" (IFCTEXT)
    URLProducto = "http://www.baxi.es/docs/sp_folleta/Folleto_EuroCondens_SGB_2013_BAXI.pdf" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Extremo inicial de nivel - Círculo: Extremo inicial de nivel - Círculo" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Nivel 1" (IFCTEXT)
    Level = "Level: Nivel 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Eurocondens SGB 215" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Baxi Calefacción, S.L.U." (IFCLABEL)
  Cantidades de equipos mecánicos | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Código de montaje = "" (IFCTEXT)
    Descripción = "Calderas de fundición de 125 kW de potencia útil, para instalaciones de Calefacción por agua caliente hasta 6 bar. Posibilidad integral de conexión doble en cascada homologada como un único generador." (IFCTEXT)
    Descripción de montaje = "" (IFCTEXT)
    Descripción de unidad = "2014_2-Calderas_Baxi_de-Gas-de-Condensación-Eurocondens-SGB-125-300-en-cascada: Eurocondens SGB 215" (IFCLABEL)
    Fabricante = "Baxi Calefacción, S.L.U." (IFCTEXT)
    Modelo = "2 calderas Eurocondens SGB 215 en cascada" (IFCTEXT)
    Tipo = "2014_2-Calderas_Baxi_de-Gas-de-Condensación-Eurocondens-SGB-125-300-en-cascada: Eurocondens SGB 215" (IFCLABEL)
    URL = "www.baxi.es" (IFCTEXT)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 20.7487034134868 (IFCAREAMEASURE) [SQUARE_METRE]
    Separación Calderas en Cascada (mm) = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 2.25573817396874 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    A-Espacio de Seguridad Recomendado = 800. (IFCLENGTHMEASURE) [MILLI METRE]
    Altura caldera (mm) = 1389. (IFCLENGTHMEASURE) [MILLI METRE]
    Ancho caldera (mm) = 692. (IFCLENGTHMEASURE) [MILLI METRE]
    B-Espacio de Seguridad Recomendado = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    C-Espacio de Seguridad Recomendado (Derecha) = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    C-Espacio de Seguridad Recomendado (Izquierda) = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    D-Espacio de Seguridad Recomendado = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Diametro Interior Entrada de Aire (mm) = 125. (IFCLENGTHMEASURE) [MILLI METRE]
    Diametro Interior Gas (mm) = 42. (IFCLENGTHMEASURE) [MILLI METRE]
    Diametro Interior IC-RC (mm) = 65. (IFCLENGTHMEASURE) [MILLI METRE]
    Diametro Interior Salida de Humos (mm) = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Diametro Interior Válvula Seguridad (mm) = 35. (IFCLENGTHMEASURE) [MILLI METRE]
    Largo caldera (mm) = 1171. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Espacio de Seguridad Recomendado = FALSE (IFCBOOLEAN)
    System Classification = "Vent,Hydronic Supply,Hydronic Return,Other,Vent,Other,Hydronic Supply,Other,Vent,Other,Vent" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Flujo Entrada Aire = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flujo Gas = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flujo Humo = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flujo Ida - Agua = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flujo Retorno - Agua = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "Fase 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Data | properties | on 1 type object
    Capacidad agua = 0.038 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Longitud máx. evacuación de humos (m) = 60. (IFCLENGTHMEASURE) [MILLI METRE]
    Peso neto aproximado = 285. (IFCREAL)
    Potencia útil 50/30 ºC = 229600. (IFCPOWERMEASURE) [WATT]
    Potencia útil 80/60 ºC = 210100. (IFCPOWERMEASURE) [WATT]
    Presión máxima de trabajo = 600000. (IFCPRESSUREMEASURE) [PASCAL]
    Rendimiento útil (1) con carga 100% = 1.068 (IFCREAL)
    Rendimiento útil (1) con carga 30% = 1.069 (IFCREAL)
    Rendimiento útil (2) con carga 100% = 0.977 (IFCREAL)
    Tipo de gas = "natural/propano" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    Carcasa = "Aleación aluminio-silicio acabado pintura - Baxi" (IFCLABEL)
    Display = "Display - Baxi" (IFCLABEL)
    Pantalla = "Cristal Display - Baxi" (IFCLABEL)
    Requerimiento de Espacio Recomendado = "Requerimiento Espacio Recomendado" (IFCLABEL)