    PAD Specification File
    ***************************

    PART TYPE:        LFXP10C
    SPEED GRADE:      5
    PACKAGE:          FPBGA388
    Package: Version 1.13.1.2, Status: PRODUCTION

    Thu Jun 23 11:37:06 2005

    Pinout by Port Name:
    +-----------------------------------------+--------------------+--------------------+--------------------------+
    |  Port Name                              |  Pin/Bank          |  Buffer Type       |  Properties              |
    +-----------------------------------------+--------------------+--------------------+--------------------------+
    | VREF1_BANK_2                            | L21/2              |                    | VREF1_DRIVER             |
    | clk_in                                  | A10/0              | LVCMOS25_IN        | SLEW:FAST                |
    | ddr_addr_0                              | R19/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_addr_1                              | R21/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_addr_10                             | T22/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_addr_11                             | M19/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_addr_12                             | M22/2              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_addr_2                              | P19/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_addr_3                              | R22/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_addr_4                              | P22/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_addr_5                              | P20/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_addr_6                              | N19/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_addr_7                              | P21/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_addr_8                              | M20/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_addr_9                              | N21/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_ba_0                                | V22/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_ba_1                                | T19/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_cas_n                               | T20/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_cke0                                | J20/2              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_cke1                                | J19/2              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_clk                                 | H19/2              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_clk_n                               | G19/2              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_cs_n1                               | U20/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_cs_n_0                              | W22/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_0                              | F21/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_1                              | E22/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_10                             | K22/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_11                             | L22/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_12                             | J21/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_13                             | K19/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_14                             | L19/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_15                             | L20/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_16                             | Y12/5              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_17                             | Y11/5              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_18                             | AB15/4             | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_19                             | AA15/4             | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_2                              | F22/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_20                             | AB13/4             | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_21                             | AB12/4             | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_22                             | A14/1              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_23                             | B15/1              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_24                             | Y18/4              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_25                             | AB17/4             | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_26                             | C12/1              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_27                             | C11/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_28                             | AA17/4             | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_29                             | AB16/4             | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_3                              | G22/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_30                             | Y13/4              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_31                             | Y14/4              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_data_4                              | D21/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_5                              | E21/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_6                              | F20/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_7                              | H20/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_8                              | H22/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_data_9                              | J22/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_dm_0                                | D22/2              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_dm_1                                | K21/2              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_dm_2                                | W2/6               | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_dm_3                                | P4/6               | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_dqs_0                               | G21/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_dqs_1                               | K20/2              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | ddr_dqs_2                               | C21/1              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_dqs_3                               | H21/2              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_ras_n                               | U19/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | ddr_we_n                                | U21/3              | SSTL25_II_OUT      | SLEW:FAST                |
    | debug_port_a_0                          | B13/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_1                          | B12/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_10                         | C3/0               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_11                         | B4/0               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_12                         | B3/0               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_13                         | A4/0               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_14                         | A3/0               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_15                         | A2/0               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_2                          | A18/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_3                          | A13/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_4                          | A12/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_5                          | D9/0               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_6                          | D8/0               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_7                          | D3/0               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_8                          | C5/0               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_9                          | C4/0               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_0                          | K4/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_1                          | J4/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_10                         | E2/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_11                         | E1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_12                         | D2/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_13                         | D1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_14                         | D12/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_15                         | B22/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_2                          | H4/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_3                          | G3/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_4                          | G2/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_5                          | G1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_6                          | F3/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_7                          | F2/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_8                          | F1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_9                          | E3/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | ledout_0                                | H1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_1                                | B16/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_2                                | B18/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_3                                | C18/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_4                                | C19/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_5                                | C20/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_6                                | W16/4              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_7                                | A16/1              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | rst_n                                   | AB2/5              | LVCMOS25_IN        | SLEW:FAST PULL:UP        |
    | vref1A                                  | A8/0               | LVCMOS25_IN        | SLEW:FAST                |
    | vref1B                                  | A17/1              | LVCMOS25_IN        | SLEW:FAST                |
    | vref1D                                  | B21/1              | LVCMOS25_IN        | SLEW:FAST                |
    | vref2A                                  | A6/0               | LVCMOS25_IN        | SLEW:FAST                |
    | vref2B                                  | R20/3              | LVCMOS25_IN        | SLEW:FAST                |
    | vref2C                                  | G20/2              | LVCMOS25_IN        | SLEW:FAST                |
    | vref2D                                  | N20/3              | LVCMOS25_IN        | SLEW:FAST                |
    +-----------------------------------------+--------------------+--------------------+--------------------------+

    Vccio by Bank:
    +--------------------+--------------------+
    |  Bank              |  Vccio             |
    +--------------------+--------------------+
    | 0                  | 2.5V               |
    | 1                  | 2.5V               |
    | 2                  | 2.5V               |
    | 3                  | 2.5V               |
    | 4                  | 2.5V               |
    | 5                  | 2.5V               |
    | 6                  | 2.5V               |
    | 7                  | 2.5V               |
    +--------------------+--------------------+

    Vref by Bank:
    +--------------------+---------+--------------------+-------------------------------+
    |  Vref              |  Pin    |  Bank # / Vref #   |  Load                         |
    +--------------------+---------+--------------------+-------------------------------+
    | VREF1_BANK_2       | L21     | 2 / VREF1 (1.25V)  | L22   K22   L19   K20   L20   |
    |                    |         |                    | J22   J21   H22   K19   H20   |
    |                    |         |                    | G22   G21   F20   F22   F21   |
    |                    |         |                    | E22   E21   D21               |
    +--------------------+---------+--------------------+-------------------------------+

    Pinout by Pin Number:
    +--------------------+--------------------+--------------------+--------------------+
    |  Pin/Bank          |  Pin Info          |  Preference        |  Buffer Type       |
    +--------------------+--------------------+--------------------+--------------------+
    | A2/0               | debug_port_a_15    |                    | LVCMOS25_OUT       |
    | A3/0               | debug_port_a_14    |                    | LVCMOS25_OUT       |
    | A4/0               | debug_port_a_13    |                    | LVCMOS25_OUT       |
    | A5/0               |                    |                    |                    |
    | A6/0               | vref2A             |                    | LVCMOS25_IN        |
    | A7/0               |                    |                    |                    |
    | A8/0               | vref1A             |                    | LVCMOS25_IN        |
    | A9/0               |                    |                    |                    |
    | A10/0              | clk_in             |                    | LVCMOS25_IN        |
    | A11/0              |                    |                    |                    |
    | A12/1              | debug_port_a_4     |                    | LVCMOS25_OUT       |
    | A13/1              | debug_port_a_3     |                    | LVCMOS25_OUT       |
    | A14/1              | ddr_data_22        |                    | SSTL25_II_OUT      |
    | A15/1              |                    |                    |                    |
    | A16/1              | ledout_7           |                    | LVCMOS25_OUT       |
    | A17/1              | vref1B             |                    | LVCMOS25_IN        |
    | A18/1              | debug_port_a_2     |                    | LVCMOS25_OUT       |
    | A19/1              |                    |                    |                    |
    | A20/1              |                    |                    |                    |
    | A21/1              |                    |                    |                    |
    | AA3/5              |                    |                    |                    |
    | AA4/5              |                    |                    |                    |
    | AA5/5              |                    |                    |                    |
    | AA6/5              |                    |                    |                    |
    | AA7/5              |                    |                    |                    |
    | AA8/5              |                    |                    |                    |
    | AA9/5              |                    |                    |                    |
    | AA10/5             |                    |                    |                    |
    | AA11/5             |                    |                    |                    |
    | AA12/4             |                    |                    |                    |
    | AA13/4             |                    |                    |                    |
    | AA14/4             |                    |                    |                    |
    | AA15/4             | ddr_data_19        |                    | SSTL25_II_OUT      |
    | AA16/4             |                    |                    |                    |
    | AA17/4             | ddr_data_28        |                    | SSTL25_II_OUT      |
    | AA18/4             |                    |                    |                    |
    | AA19/4             |                    |                    |                    |
    | AA20/4             |                    |                    |                    |
    | AA21/4             |                    |                    |                    |
    | AA22/4             |                    |                    |                    |
    | AB2/5              | rst_n              |                    | LVCMOS25_IN        |
    | AB3/5              |                    |                    |                    |
    | AB4/5              |                    |                    |                    |
    | AB5/5              |                    |                    |                    |
    | AB6/5              |                    |                    |                    |
    | AB7/5              |                    |                    |                    |
    | AB8/5              |                    |                    |                    |
    | AB9/5              |                    |                    |                    |
    | AB10/5             |                    |                    |                    |
    | AB11/5             |                    |                    |                    |
    | AB12/4             | ddr_data_21        |                    | SSTL25_II_OUT      |
    | AB13/4             | ddr_data_20        |                    | SSTL25_II_OUT      |
    | AB14/4             |                    |                    |                    |
    | AB15/4             | ddr_data_18        |                    | SSTL25_II_OUT      |
    | AB16/4             | ddr_data_29        |                    | SSTL25_II_OUT      |
    | AB17/4             | ddr_data_25        |                    | SSTL25_II_OUT      |
    | AB18/4             |                    |                    |                    |
    | AB19/4             |                    |                    |                    |
    | AB20/4             |                    |                    |                    |
    | AB21/4             |                    |                    |                    |
    | B3/0               | debug_port_a_12    |                    | LVCMOS25_OUT       |
    | B4/0               | debug_port_a_11    |                    | LVCMOS25_OUT       |
    | B5/0               |                    |                    |                    |
    | B6/0               |                    |                    |                    |
    | B7/0               |                    |                    |                    |
    | B8/0               |                    |                    |                    |
    | B9/0               |                    |                    |                    |
    | B10/0              |                    |                    |                    |
    | B11/0              |                    |                    |                    |
    | B12/1              | debug_port_a_1     |                    | LVCMOS25_OUT       |
    | B13/1              | debug_port_a_0     |                    | LVCMOS25_OUT       |
    | B14/1              |                    |                    |                    |
    | B15/1              | ddr_data_23        |                    | SSTL25_II_OUT      |
    | B16/1              | ledout_1           |                    | LVCMOS25_OUT       |
    | B17/1              |                    |                    |                    |
    | B18/1              | ledout_2           |                    | LVCMOS25_OUT       |
    | B19/1              |                    |                    |                    |
    | B20/1              |                    |                    |                    |
    | B21/1              | vref1D             |                    | LVCMOS25_IN        |
    | B22/1              | debug_port_b_15    |                    | LVCMOS25_OUT       |
    | C3/0               | debug_port_a_10    |                    | LVCMOS25_OUT       |
    | C4/0               | debug_port_a_9     |                    | LVCMOS25_OUT       |
    | C5/0               | debug_port_a_8     |                    | LVCMOS25_OUT       |
    | C6/0               |                    |                    |                    |
    | C7/0               |                    |                    |                    |
    | C8/0               |                    |                    |                    |
    | C9/0               |                    |                    |                    |
    | C10/0              |                    |                    |                    |
    | C11/0              | ddr_data_27        |                    | SSTL25_II_OUT      |
    | C12/1              | ddr_data_26        |                    | SSTL25_II_OUT      |
    | C13/1              |                    |                    |                    |
    | C14/1              |                    |                    |                    |
    | C18/1              | ledout_3           |                    | LVCMOS25_OUT       |
    | C19/1              | ledout_4           |                    | LVCMOS25_OUT       |
    | C20/1              | ledout_5           |                    | LVCMOS25_OUT       |
    | C21/1              | ddr_dqs_2          |                    | SSTL25_II_OUT      |
    | C22/1              |                    |                    |                    |
    | D1/7               | debug_port_b_13    |                    | LVCMOS25_OUT       |
    | D2/7               | debug_port_b_12    |                    | LVCMOS25_OUT       |
    | D3/0               | debug_port_a_7     |                    | LVCMOS25_OUT       |
    | D8/0               | debug_port_a_6     |                    | LVCMOS25_OUT       |
    | D9/0               | debug_port_a_5     |                    | LVCMOS25_OUT       |
    | D10/0              |                    |                    |                    |
    | D11/0              |                    |                    |                    |
    | D12/1              | debug_port_b_14    |                    | LVCMOS25_OUT       |
    | D13/1              |                    |                    |                    |
    | D14/1              |                    |                    |                    |
    | D15/1              |                    |                    |                    |
    | D21/2              | ddr_data_4         |                    | SSTL25_II_BIDI     |
    | D22/2              | ddr_dm_0           |                    | SSTL25_II_OUT      |
    | E1/7               | debug_port_b_11    |                    | LVCMOS25_OUT       |
    | E2/7               | debug_port_b_10    |                    | LVCMOS25_OUT       |
    | E3/7               | debug_port_b_9     |                    | LVCMOS25_OUT       |
    | E21/2              | ddr_data_5         |                    | SSTL25_II_BIDI     |
    | E22/2              | ddr_data_1         |                    | SSTL25_II_BIDI     |
    | F1/7               | debug_port_b_8     |                    | LVCMOS25_OUT       |
    | F2/7               | debug_port_b_7     |                    | LVCMOS25_OUT       |
    | F3/7               | debug_port_b_6     |                    | LVCMOS25_OUT       |
    | F20/2              | ddr_data_6         |                    | SSTL25_II_BIDI     |
    | F21/2              | ddr_data_0         |                    | SSTL25_II_BIDI     |
    | F22/2              | ddr_data_2         |                    | SSTL25_II_BIDI     |
    | G1/7               | debug_port_b_5     |                    | LVCMOS25_OUT       |
    | G2/7               | debug_port_b_4     |                    | LVCMOS25_OUT       |
    | G3/7               | debug_port_b_3     |                    | LVCMOS25_OUT       |
    | G19/2              | ddr_clk_n          |                    | SSTL25_II_OUT      |
    | G20/2              | vref2C             |                    | LVCMOS25_IN        |
    | G21/2              | ddr_dqs_0          |                    | SSTL25_II_BIDI     |
    | G22/2              | ddr_data_3         |                    | SSTL25_II_BIDI     |
    | H1/7               | ledout_0           |                    | LVCMOS25_OUT       |
    | H2/7               |                    |                    |                    |
    | H3/7               |                    |                    |                    |
    | H4/7               | debug_port_b_2     |                    | LVCMOS25_OUT       |
    | H19/2              | ddr_clk            |                    | SSTL25_II_OUT      |
    | H20/2              | ddr_data_7         |                    | SSTL25_II_BIDI     |
    | H21/2              | ddr_dqs_3          |                    | SSTL25_II_OUT      |
    | H22/2              | ddr_data_8         |                    | SSTL25_II_BIDI     |
    | J1/7               |                    |                    |                    |
    | J2/7               |                    |                    |                    |
    | J3/7               |                    |                    |                    |
    | J4/7               | debug_port_b_1     |                    | LVCMOS25_OUT       |
    | J19/2              | ddr_cke1           |                    | SSTL25_II_OUT      |
    | J20/2              | ddr_cke0           |                    | SSTL25_II_OUT      |
    | J21/2              | ddr_data_12        |                    | SSTL25_II_BIDI     |
    | J22/2              | ddr_data_9         |                    | SSTL25_II_BIDI     |
    | K1/7               |                    |                    |                    |
    | K2/7               |                    |                    |                    |
    | K3/7               |                    |                    |                    |
    | K4/7               | debug_port_b_0     |                    | LVCMOS25_OUT       |
    | K19/2              | ddr_data_13        |                    | SSTL25_II_BIDI     |
    | K20/2              | ddr_dqs_1          |                    | SSTL25_II_BIDI     |
    | K21/2              | ddr_dm_1           |                    | SSTL25_II_OUT      |
    | K22/2              | ddr_data_10        |                    | SSTL25_II_BIDI     |
    | L1/7               |                    |                    |                    |
    | L2/7               |                    |                    |                    |
    | L3/7               |                    |                    |                    |
    | L4/7               |                    |                    |                    |
    | L19/2              | ddr_data_14        |                    | SSTL25_II_BIDI     |
    | L20/2              | ddr_data_15        |                    | SSTL25_II_BIDI     |
    | L21/2              | VREF1_BANK_2       |                    |                    |
    | L22/2              | ddr_data_11        |                    | SSTL25_II_BIDI     |
    | M1/7               |                    |                    |                    |
    | M3/6               |                    |                    |                    |
    | M4/6               |                    |                    |                    |
    | M19/3              | ddr_addr_11        |                    | SSTL25_II_OUT      |
    | M20/3              | ddr_addr_8         |                    | SSTL25_II_OUT      |
    | M22/2              | ddr_addr_12        |                    | SSTL25_II_OUT      |
    | N2/6               |                    |                    |                    |
    | N3/6               |                    |                    |                    |
    | N4/6               |                    |                    |                    |
    | N19/3              | ddr_addr_6         |                    | SSTL25_II_OUT      |
    | N20/3              | vref2D             |                    | LVCMOS25_IN        |
    | N21/3              | ddr_addr_9         |                    | SSTL25_II_OUT      |
    | P1/6               |                    |                    |                    |
    | P2/6               |                    |                    |                    |
    | P3/6               |                    |                    |                    |
    | P4/6               | ddr_dm_3           |                    | SSTL25_II_OUT      |
    | P19/3              | ddr_addr_2         |                    | SSTL25_II_OUT      |
    | P20/3              | ddr_addr_5         |                    | SSTL25_II_OUT      |
    | P21/3              | ddr_addr_7         |                    | SSTL25_II_OUT      |
    | P22/3              | ddr_addr_4         |                    | SSTL25_II_OUT      |
    | PB2B/0             |                    |                    |                    |
    | PB8B/0             |                    |                    |                    |
    | PB9A/0             |                    |                    |                    |
    | PB16B/0            |                    |                    |                    |
    | PB17A/0            |                    |                    |                    |
    | PB24B/0            |                    |                    |                    |
    | PB25A/0            |                    |                    |                    |
    | PB32B/0            |                    |                    |                    |
    | PB33A/0            |                    |                    |                    |
    | PB39B/0            |                    |                    |                    |
    | PL5B/0             |                    |                    |                    |
    | PL6A/0             |                    |                    |                    |
    | PL14B/0            |                    |                    |                    |
    | PL15A/0            |                    |                    |                    |
    | PL22B/0            |                    |                    |                    |
    | PL23A/0            |                    |                    |                    |
    | PL31B/0            |                    |                    |                    |
    | PL32A/0            |                    |                    |                    |
    | PR5B/0             |                    |                    |                    |
    | PR6A/0             |                    |                    |                    |
    | PR14B/0            |                    |                    |                    |
    | PR15A/0            |                    |                    |                    |
    | PR22B/0            |                    |                    |                    |
    | PR23A/0            |                    |                    |                    |
    | PR31B/0            |                    |                    |                    |
    | PR32A/0            |                    |                    |                    |
    | PT2B/0             |                    |                    |                    |
    | PT8B/0             |                    |                    |                    |
    | PT9A/0             |                    |                    |                    |
    | PT16B/0            |                    |                    |                    |
    | PT17A/0            |                    |                    |                    |
    | PT24B/0            |                    |                    |                    |
    | PT25A/0            |                    |                    |                    |
    | PT32B/0            |                    |                    |                    |
    | PT33A/0            |                    |                    |                    |
    | PT39B/0            |                    |                    |                    |
    | R1/6               |                    |                    |                    |
    | R2/6               |                    |                    |                    |
    | R3/6               |                    |                    |                    |
    | R4/6               |                    |                    |                    |
    | R19/3              | ddr_addr_0         |                    | SSTL25_II_OUT      |
    | R20/3              | vref2B             |                    | LVCMOS25_IN        |
    | R21/3              | ddr_addr_1         |                    | SSTL25_II_OUT      |
    | R22/3              | ddr_addr_3         |                    | SSTL25_II_OUT      |
    | T1/6               |                    |                    |                    |
    | T2/6               |                    |                    |                    |
    | T3/6               |                    |                    |                    |
    | T4/6               |                    |                    |                    |
    | T19/3              | ddr_ba_1           |                    | SSTL25_II_OUT      |
    | T20/3              | ddr_cas_n          |                    | SSTL25_II_OUT      |
    | T21/3              |                    |                    |                    |
    | T22/3              | ddr_addr_10        |                    | SSTL25_II_OUT      |
    | TCK/1              |                    |                    |                    |
    | TDI/1              |                    |                    |                    |
    | TDO/2              |                    |                    |                    |
    | TMS/1              |                    |                    |                    |
    | U1/6               |                    |                    |                    |
    | U2/6               |                    |                    |                    |
    | U3/6               |                    |                    |                    |
    | U4/6               |                    |                    |                    |
    | U19/3              | ddr_ras_n          |                    | SSTL25_II_OUT      |
    | U20/3              | ddr_cs_n1          |                    | SSTL25_II_OUT      |
    | U21/3              | ddr_we_n           |                    | SSTL25_II_OUT      |
    | U22/3              |                    |                    |                    |
    | V1/6               |                    |                    |                    |
    | V2/6               |                    |                    |                    |
    | V3/6               |                    |                    |                    |
    | V4/6               |                    |                    |                    |
    | V19/3              |                    |                    |                    |
    | V20/3              |                    |                    |                    |
    | V21/3              |                    |                    |                    |
    | V22/3              | ddr_ba_0           |                    | SSTL25_II_OUT      |
    | W1/6               |                    |                    |                    |
    | W2/6               | ddr_dm_2           |                    | SSTL25_II_OUT      |
    | W6/5               |                    |                    |                    |
    | W8/5               |                    |                    |                    |
    | W9/5               |                    |                    |                    |
    | W10/5              |                    |                    |                    |
    | W11/5              |                    |                    |                    |
    | W12/4              |                    |                    |                    |
    | W13/4              |                    |                    |                    |
    | W14/4              |                    |                    |                    |
    | W15/4              |                    |                    |                    |
    | W16/4              | ledout_6           |                    | LVCMOS25_OUT       |
    | W21/3              |                    |                    |                    |
    | W22/3              | ddr_cs_n_0         |                    | SSTL25_II_OUT      |
    | Y1/6               |                    |                    |                    |
    | Y4/5               |                    |                    |                    |
    | Y5/5               |                    |                    |                    |
    | Y6/5               |                    |                    |                    |
    | Y7/5               |                    |                    |                    |
    | Y8/5               |                    |                    |                    |
    | Y9/5               |                    |                    |                    |
    | Y10/5              |                    |                    |                    |
    | Y11/5              | ddr_data_17        |                    | SSTL25_II_OUT      |
    | Y12/5              | ddr_data_16        |                    | SSTL25_II_OUT      |
    | Y13/4              | ddr_data_30        |                    | SSTL25_II_OUT      |
    | Y14/4              | ddr_data_31        |                    | SSTL25_II_OUT      |
    | Y17/4              |                    |                    |                    |
    | Y18/4              | ddr_data_24        |                    | SSTL25_II_OUT      |
    | Y19/4              |                    |                    |                    |
    | Y20/4              |                    |                    |                    |
    | Y21/4              |                    |                    |                    |
    | Y22/3              |                    |                    |                    |
    +--------------------+--------------------+--------------------+--------------------+

    Locate Preferences for each Pin:

    LOCATE  COMP  "clk_in"  SITE  "A10";
    LOCATE  COMP  "ddr_addr_0"  SITE  "R19";
    LOCATE  COMP  "ddr_addr_1"  SITE  "R21";
    LOCATE  COMP  "ddr_addr_10"  SITE  "T22";
    LOCATE  COMP  "ddr_addr_11"  SITE  "M19";
    LOCATE  COMP  "ddr_addr_12"  SITE  "M22";
    LOCATE  COMP  "ddr_addr_2"  SITE  "P19";
    LOCATE  COMP  "ddr_addr_3"  SITE  "R22";
    LOCATE  COMP  "ddr_addr_4"  SITE  "P22";
    LOCATE  COMP  "ddr_addr_5"  SITE  "P20";
    LOCATE  COMP  "ddr_addr_6"  SITE  "N19";
    LOCATE  COMP  "ddr_addr_7"  SITE  "P21";
    LOCATE  COMP  "ddr_addr_8"  SITE  "M20";
    LOCATE  COMP  "ddr_addr_9"  SITE  "N21";
    LOCATE  COMP  "ddr_ba_0"  SITE  "V22";
    LOCATE  COMP  "ddr_ba_1"  SITE  "T19";
    LOCATE  COMP  "ddr_cas_n"  SITE  "T20";
    LOCATE  COMP  "ddr_cke0"  SITE  "J20";
    LOCATE  COMP  "ddr_cke1"  SITE  "J19";
    LOCATE  COMP  "ddr_clk"  SITE  "H19";
    LOCATE  COMP  "ddr_clk_n"  SITE  "G19";
    LOCATE  COMP  "ddr_cs_n1"  SITE  "U20";
    LOCATE  COMP  "ddr_cs_n_0"  SITE  "W22";
    LOCATE  COMP  "ddr_data_0"  SITE  "F21";
    LOCATE  COMP  "ddr_data_1"  SITE  "E22";
    LOCATE  COMP  "ddr_data_10"  SITE  "K22";
    LOCATE  COMP  "ddr_data_11"  SITE  "L22";
    LOCATE  COMP  "ddr_data_12"  SITE  "J21";
    LOCATE  COMP  "ddr_data_13"  SITE  "K19";
    LOCATE  COMP  "ddr_data_14"  SITE  "L19";
    LOCATE  COMP  "ddr_data_15"  SITE  "L20";
    LOCATE  COMP  "ddr_data_16"  SITE  "Y12";
    LOCATE  COMP  "ddr_data_17"  SITE  "Y11";
    LOCATE  COMP  "ddr_data_18"  SITE  "AB15";
    LOCATE  COMP  "ddr_data_19"  SITE  "AA15";
    LOCATE  COMP  "ddr_data_2"  SITE  "F22";
    LOCATE  COMP  "ddr_data_20"  SITE  "AB13";
    LOCATE  COMP  "ddr_data_21"  SITE  "AB12";
    LOCATE  COMP  "ddr_data_22"  SITE  "A14";
    LOCATE  COMP  "ddr_data_23"  SITE  "B15";
    LOCATE  COMP  "ddr_data_24"  SITE  "Y18";
    LOCATE  COMP  "ddr_data_25"  SITE  "AB17";
    LOCATE  COMP  "ddr_data_26"  SITE  "C12";
    LOCATE  COMP  "ddr_data_27"  SITE  "C11";
    LOCATE  COMP  "ddr_data_28"  SITE  "AA17";
    LOCATE  COMP  "ddr_data_29"  SITE  "AB16";
    LOCATE  COMP  "ddr_data_3"  SITE  "G22";
    LOCATE  COMP  "ddr_data_30"  SITE  "Y13";
    LOCATE  COMP  "ddr_data_31"  SITE  "Y14";
    LOCATE  COMP  "ddr_data_4"  SITE  "D21";
    LOCATE  COMP  "ddr_data_5"  SITE  "E21";
    LOCATE  COMP  "ddr_data_6"  SITE  "F20";
    LOCATE  COMP  "ddr_data_7"  SITE  "H20";
    LOCATE  COMP  "ddr_data_8"  SITE  "H22";
    LOCATE  COMP  "ddr_data_9"  SITE  "J22";
    LOCATE  COMP  "ddr_dm_0"  SITE  "D22";
    LOCATE  COMP  "ddr_dm_1"  SITE  "K21";
    LOCATE  COMP  "ddr_dm_2"  SITE  "W2";
    LOCATE  COMP  "ddr_dm_3"  SITE  "P4";
    LOCATE  COMP  "ddr_dqs_0"  SITE  "G21";
    LOCATE  COMP  "ddr_dqs_1"  SITE  "K20";
    LOCATE  COMP  "ddr_dqs_2"  SITE  "C21";
    LOCATE  COMP  "ddr_dqs_3"  SITE  "H21";
    LOCATE  COMP  "ddr_ras_n"  SITE  "U19";
    LOCATE  COMP  "ddr_we_n"  SITE  "U21";
    LOCATE  COMP  "debug_port_a_0"  SITE  "B13";
    LOCATE  COMP  "debug_port_a_1"  SITE  "B12";
    LOCATE  COMP  "debug_port_a_10"  SITE  "C3";
    LOCATE  COMP  "debug_port_a_11"  SITE  "B4";
    LOCATE  COMP  "debug_port_a_12"  SITE  "B3";
    LOCATE  COMP  "debug_port_a_13"  SITE  "A4";
    LOCATE  COMP  "debug_port_a_14"  SITE  "A3";
    LOCATE  COMP  "debug_port_a_15"  SITE  "A2";
    LOCATE  COMP  "debug_port_a_2"  SITE  "A18";
    LOCATE  COMP  "debug_port_a_3"  SITE  "A13";
    LOCATE  COMP  "debug_port_a_4"  SITE  "A12";
    LOCATE  COMP  "debug_port_a_5"  SITE  "D9";
    LOCATE  COMP  "debug_port_a_6"  SITE  "D8";
    LOCATE  COMP  "debug_port_a_7"  SITE  "D3";
    LOCATE  COMP  "debug_port_a_8"  SITE  "C5";
    LOCATE  COMP  "debug_port_a_9"  SITE  "C4";
    LOCATE  COMP  "debug_port_b_0"  SITE  "K4";
    LOCATE  COMP  "debug_port_b_1"  SITE  "J4";
    LOCATE  COMP  "debug_port_b_10"  SITE  "E2";
    LOCATE  COMP  "debug_port_b_11"  SITE  "E1";
    LOCATE  COMP  "debug_port_b_12"  SITE  "D2";
    LOCATE  COMP  "debug_port_b_13"  SITE  "D1";
    LOCATE  COMP  "debug_port_b_14"  SITE  "D12";
    LOCATE  COMP  "debug_port_b_15"  SITE  "B22";
    LOCATE  COMP  "debug_port_b_2"  SITE  "H4";
    LOCATE  COMP  "debug_port_b_3"  SITE  "G3";
    LOCATE  COMP  "debug_port_b_4"  SITE  "G2";
    LOCATE  COMP  "debug_port_b_5"  SITE  "G1";
    LOCATE  COMP  "debug_port_b_6"  SITE  "F3";
    LOCATE  COMP  "debug_port_b_7"  SITE  "F2";
    LOCATE  COMP  "debug_port_b_8"  SITE  "F1";
    LOCATE  COMP  "debug_port_b_9"  SITE  "E3";
    LOCATE  COMP  "ledout_0"  SITE  "H1";
    LOCATE  COMP  "ledout_1"  SITE  "B16";
    LOCATE  COMP  "ledout_2"  SITE  "B18";
    LOCATE  COMP  "ledout_3"  SITE  "C18";
    LOCATE  COMP  "ledout_4"  SITE  "C19";
    LOCATE  COMP  "ledout_5"  SITE  "C20";
    LOCATE  COMP  "ledout_6"  SITE  "W16";
    LOCATE  COMP  "ledout_7"  SITE  "A16";
    LOCATE  COMP  "rst_n"  SITE  "AB2";
    LOCATE  COMP  "vref1A"  SITE  "A8";
    LOCATE  COMP  "vref1B"  SITE  "A17";
    LOCATE  COMP  "vref1D"  SITE  "B21";
    LOCATE  COMP  "vref2A"  SITE  "A6";
    LOCATE  COMP  "vref2B"  SITE  "R20";
    LOCATE  COMP  "vref2C"  SITE  "G20";
    LOCATE  COMP  "vref2D"  SITE  "N20";

    #DQSDLL
    LOCATE  COMP  "U1_ddr_sdram_mem_top/U1_DQSDLL"  SITE  "TDLL" ;
    #PLL
    LOCATE  COMP  "U1_ddr_sdram_mem_top/U1_kbar_clk_pll/U1_PLL"  SITE  "PLL3_R27C1" ;

    LOCATE  VREF  "VREF1_BANK_2"  SITE  "L21"  LEVELMODE  "SSTL25_II_BIDI";

    PAR: Place And Route ispLever_v50_Production_Build (40).
    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
    Copyright (c) 1995 AT&T Corp.   All rights reserved.
    Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
    Copyright (c) 2001 Agere Systems   All rights reserved.
    Copyright (c) 2002-2005 Lattice Semiconductor Corporation,  All rights reserved.
    Thu Jun 23 11:37:06 2005

    Generated from the file 'C:\EVALUATION BOARDS\XP\HIGH_END\EVAL_CODE\DDR\VHDL\PNR\ddr_vhdl_pnr.pad'