    PAD Specification File
    ***************************

    PART TYPE:        LFEC20E
    SPEED GRADE:      5
    PACKAGE:          FPBGA672
    Package: Version 1.8, Status: PRODUCTION

    Wed Jun 29 14:21:51 2005

    Pinout by Port Name:
    +-----------------------------------------+--------------------+--------------------+--------------------------+
    |  Port Name                              |  Pin/Bank          |  Buffer Type       |  Properties              |
    +-----------------------------------------+--------------------+--------------------+--------------------------+
    | VREF1_BANK_0                            | D13/0              |                    | VREF1_DRIVER             |
    | clk_in                                  | F6/7               | LVCMOS25_IN        | SLEW:FAST                |
    | debug_port_a_0                          | AE4/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_1                          | AE5/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_10                         | AD7/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_11                         | AD8/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_12                         | AD9/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_13                         | AD10/5             | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_14                         | AD11/5             | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_15                         | AD12/5             | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_2                          | AE6/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_3                          | AE7/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_4                          | AE8/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_5                          | AE9/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_6                          | AE10/5             | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_7                          | AD4/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_8                          | AD5/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_a_9                          | AD6/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_0                          | AF4/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_1                          | AF5/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_10                         | AC6/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_11                         | AC7/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_12                         | AC8/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_13                         | AC9/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_14                         | AC10/5             | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_15                         | AC11/5             | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_2                          | AF6/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_3                          | AF7/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_4                          | AF8/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_5                          | AF9/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_6                          | AF10/5             | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_7                          | AF11/5             | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_8                          | AC4/6              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_b_9                          | AC5/5              | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_0                          | U4/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_1                          | U3/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_10                         | R2/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_11                         | R1/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_12                         | P4/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_13                         | P3/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_14                         | P2/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_15                         | P1/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_16                         | U5/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_17                         | T5/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_18                         | R5/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_19                         | P5/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_2                          | U2/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_3                          | U1/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_4                          | T4/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_5                          | T3/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_6                          | T2/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_7                          | T1/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_8                          | R4/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | debug_port_c_9                          | R3/6               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST PULL:UP
    | fcram_addr_0                            | D10/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_1                            | A9/0               | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_10                           | C10/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_11                           | G12/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_12                           | E12/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_13                           | B11/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_14                           | A11/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_2                            | B9/0               | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_3                            | C9/0               | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_4                            | G10/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_5                            | F10/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_6                            | E10/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_7                            | G11/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_8                            | F11/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_addr_9                            | E11/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_ba_0                              | A10/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_ba_1                              | B10/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_clk                               | A2/0               | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_clkn                              | A3/0               | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_csn                               | D11/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_dq_0                              | A14/0              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | fcram_dq_1                              | B14/0              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | fcram_dq_2                              | A13/0              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | fcram_dq_3                              | B13/0              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | fcram_dq_4                              | D12/0              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | fcram_dq_5                              | C12/0              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | fcram_dq_6                              | A12/0              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | fcram_dq_7                              | B12/0              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | fcram_dqs_0                             | F12/0              | SSTL25_II_BIDI     | SLEW:FAST VREF1_LOAD     |
    | fcram_fn                                | C11/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | fcram_pdn                               | F13/0              | SSTL25_II_OUT      | SLEW:FAST                |
    | ledout_0                                | B1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_1                                | C1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_2                                | D1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_3                                | E1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_4                                | F1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_5                                | G1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_6                                | H1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | ledout_7                                | J1/7               | LVCMOS25_OUT       | DRIVE:12mA SLEW:FAST     |
    | rst_n                                   | K1/7               | LVCMOS25_IN        | SLEW:FAST PULL:UP        |
    | vref1A                                  | E13/1              | LVCMOS12_IN        | SLEW:FAST                |
    | vref1B                                  | C13/0              | LVCMOS12_IN        | SLEW:FAST                |
    | vref2A                                  | D14/1              | LVCMOS12_IN        | SLEW:FAST                |
    | vref2B                                  | AF3/5              | LVCMOS12_IN        | SLEW:FAST                |
    +-----------------------------------------+--------------------+--------------------+--------------------------+

    Vccio by Bank:
    +--------------------+--------------------+
    |  Bank              |  Vccio             |
    +--------------------+--------------------+
    | 0                  | 2.5V               |
    | 5                  | 2.5V               |
    | 6                  | 2.5V               |
    | 7                  | 2.5V               |
    +--------------------+--------------------+

    Vref by Bank:
    +--------------------+---------+--------------------+-------------------------------+
    |  Vref              |  Pin    |  Bank # / Vref #   |  Load                         |
    +--------------------+---------+--------------------+-------------------------------+
    | VREF1_BANK_0       | D13     | 0 / VREF1 (1.25V)  | C12   D12   B12   A12   F12   |
    |                    |         |                    | B13   A13   A14   B14         |
    +--------------------+---------+--------------------+-------------------------------+

    Pinout by Pin Number:
    +--------------------+--------------------+--------------------+--------------------+
    |  Pin/Bank          |  Pin Info          |  Preference        |  Buffer Type       |
    +--------------------+--------------------+--------------------+--------------------+
    | A2/0               | fcram_clk          |                    | SSTL25_II_OUT      |
    | A3/0               | fcram_clkn         |                    | SSTL25_II_OUT      |
    | A4/0               |                    |                    |                    |
    | A5/0               |                    |                    |                    |
    | A6/0               |                    |                    |                    |
    | A7/0               |                    |                    |                    |
    | A8/0               |                    |                    |                    |
    | A9/0               | fcram_addr_1       |                    | SSTL25_II_OUT      |
    | A10/0              | fcram_ba_0         |                    | SSTL25_II_OUT      |
    | A11/0              | fcram_addr_14      |                    | SSTL25_II_OUT      |
    | A12/0              | fcram_dq_6         |                    | SSTL25_II_BIDI     |
    | A13/0              | fcram_dq_2         |                    | SSTL25_II_BIDI     |
    | A14/0              | fcram_dq_0         |                    | SSTL25_II_BIDI     |
    | A15/1              |                    |                    |                    |
    | A16/1              |                    |                    |                    |
    | A17/1              |                    |                    |                    |
    | A18/1              |                    |                    |                    |
    | A19/1              |                    |                    |                    |
    | A20/1              |                    |                    |                    |
    | A21/1              |                    |                    |                    |
    | A22/1              |                    |                    |                    |
    | A23/1              |                    |                    |                    |
    | A24/1              |                    |                    |                    |
    | AA1/6              |                    |                    |                    |
    | AA6/5              |                    |                    |                    |
    | AA7/5              |                    |                    |                    |
    | AA8/5              |                    |                    |                    |
    | AA9/5              |                    |                    |                    |
    | AA10/5             |                    |                    |                    |
    | AA11/5             |                    |                    |                    |
    | AA12/5             |                    |                    |                    |
    | AA13/4             |                    |                    |                    |
    | AA14/4             |                    |                    |                    |
    | AA15/4             |                    |                    |                    |
    | AA16/4             |                    |                    |                    |
    | AA17/4             |                    |                    |                    |
    | AA18/4             |                    |                    |                    |
    | AA19/4             |                    |                    |                    |
    | AA20/4             |                    |                    |                    |
    | AA25/3             |                    |                    |                    |
    | AA26/3             |                    |                    |                    |
    | AB1/6              |                    |                    |                    |
    | AB2/6              |                    |                    |                    |
    | AB4/6              |                    |                    |                    |
    | AB6/5              |                    |                    |                    |
    | AB7/5              |                    |                    |                    |
    | AB8/5              |                    |                    |                    |
    | AB9/5              |                    |                    |                    |
    | AB10/5             |                    |                    |                    |
    | AB11/5             |                    |                    |                    |
    | AB12/5             |                    |                    |                    |
    | AB13/4             |                    |                    |                    |
    | AB14/4             |                    |                    |                    |
    | AB15/4             |                    |                    |                    |
    | AB16/4             |                    |                    |                    |
    | AB17/4             |                    |                    |                    |
    | AB18/4             |                    |                    |                    |
    | AB25/3             |                    |                    |                    |
    | AB26/3             |                    |                    |                    |
    | AC1/6              |                    |                    |                    |
    | AC4/6              | debug_port_b_8     |                    | LVCMOS25_OUT       |
    | AC5/5              | debug_port_b_9     |                    | LVCMOS25_OUT       |
    | AC6/5              | debug_port_b_10    |                    | LVCMOS25_OUT       |
    | AC7/5              | debug_port_b_11    |                    | LVCMOS25_OUT       |
    | AC8/5              | debug_port_b_12    |                    | LVCMOS25_OUT       |
    | AC9/5              | debug_port_b_13    |                    | LVCMOS25_OUT       |
    | AC10/5             | debug_port_b_14    |                    | LVCMOS25_OUT       |
    | AC11/5             | debug_port_b_15    |                    | LVCMOS25_OUT       |
    | AC12/5             |                    |                    |                    |
    | AC13/5             |                    |                    |                    |
    | AC14/4             |                    |                    |                    |
    | AC15/4             |                    |                    |                    |
    | AC16/4             |                    |                    |                    |
    | AC17/4             |                    |                    |                    |
    | AC18/4             |                    |                    |                    |
    | AC23/3             |                    |                    |                    |
    | AC24/3             |                    |                    |                    |
    | AC25/3             |                    |                    |                    |
    | AC26/3             |                    |                    |                    |
    | AD4/5              | debug_port_a_7     |                    | LVCMOS25_OUT       |
    | AD5/5              | debug_port_a_8     |                    | LVCMOS25_OUT       |
    | AD6/5              | debug_port_a_9     |                    | LVCMOS25_OUT       |
    | AD7/5              | debug_port_a_10    |                    | LVCMOS25_OUT       |
    | AD8/5              | debug_port_a_11    |                    | LVCMOS25_OUT       |
    | AD9/5              | debug_port_a_12    |                    | LVCMOS25_OUT       |
    | AD10/5             | debug_port_a_13    |                    | LVCMOS25_OUT       |
    | AD11/5             | debug_port_a_14    |                    | LVCMOS25_OUT       |
    | AD12/5             | debug_port_a_15    |                    | LVCMOS25_OUT       |
    | AD13/5             |                    |                    |                    |
    | AD14/4             |                    |                    |                    |
    | AD15/4             |                    |                    |                    |
    | AD16/4             |                    |                    |                    |
    | AD17/4             |                    |                    |                    |
    | AD18/4             |                    |                    |                    |
    | AE2/5              |                    |                    |                    |
    | AE3/5              |                    |                    |                    |
    | AE4/5              | debug_port_a_0     |                    | LVCMOS25_OUT       |
    | AE5/5              | debug_port_a_1     |                    | LVCMOS25_OUT       |
    | AE6/5              | debug_port_a_2     |                    | LVCMOS25_OUT       |
    | AE7/5              | debug_port_a_3     |                    | LVCMOS25_OUT       |
    | AE8/5              | debug_port_a_4     |                    | LVCMOS25_OUT       |
    | AE9/5              | debug_port_a_5     |                    | LVCMOS25_OUT       |
    | AE10/5             | debug_port_a_6     |                    | LVCMOS25_OUT       |
    | AE11/5             |                    |                    |                    |
    | AE12/5             |                    |                    |                    |
    | AE13/5             |                    |                    |                    |
    | AE14/5             |                    |                    |                    |
    | AE15/4             |                    |                    |                    |
    | AE16/4             |                    |                    |                    |
    | AE17/4             |                    |                    |                    |
    | AE18/4             |                    |                    |                    |
    | AE19/4             |                    |                    |                    |
    | AE20/4             |                    |                    |                    |
    | AE21/4             |                    |                    |                    |
    | AE22/4             |                    |                    |                    |
    | AE23/4             |                    |                    |                    |
    | AF2/5              |                    |                    |                    |
    | AF3/5              | vref2B             |                    | LVCMOS12_IN        |
    | AF4/5              | debug_port_b_0     |                    | LVCMOS25_OUT       |
    | AF5/5              | debug_port_b_1     |                    | LVCMOS25_OUT       |
    | AF6/5              | debug_port_b_2     |                    | LVCMOS25_OUT       |
    | AF7/5              | debug_port_b_3     |                    | LVCMOS25_OUT       |
    | AF8/5              | debug_port_b_4     |                    | LVCMOS25_OUT       |
    | AF9/5              | debug_port_b_5     |                    | LVCMOS25_OUT       |
    | AF10/5             | debug_port_b_6     |                    | LVCMOS25_OUT       |
    | AF11/5             | debug_port_b_7     |                    | LVCMOS25_OUT       |
    | AF12/5             |                    |                    |                    |
    | AF13/5             |                    |                    |                    |
    | AF14/5             |                    |                    |                    |
    | AF15/4             |                    |                    |                    |
    | AF16/4             |                    |                    |                    |
    | AF17/4             |                    |                    |                    |
    | AF18/4             |                    |                    |                    |
    | AF19/4             |                    |                    |                    |
    | AF20/4             |                    |                    |                    |
    | AF21/4             |                    |                    |                    |
    | AF22/4             |                    |                    |                    |
    | AF23/4             |                    |                    |                    |
    | AF24/4             |                    |                    |                    |
    | B1/7               | ledout_0           |                    | LVCMOS25_OUT       |
    | B3/0               |                    |                    |                    |
    | B4/0               |                    |                    |                    |
    | B5/0               |                    |                    |                    |
    | B6/0               |                    |                    |                    |
    | B7/0               |                    |                    |                    |
    | B8/0               |                    |                    |                    |
    | B9/0               | fcram_addr_2       |                    | SSTL25_II_OUT      |
    | B10/0              | fcram_ba_1         |                    | SSTL25_II_OUT      |
    | B11/0              | fcram_addr_13      |                    | SSTL25_II_OUT      |
    | B12/0              | fcram_dq_7         |                    | SSTL25_II_BIDI     |
    | B13/0              | fcram_dq_3         |                    | SSTL25_II_BIDI     |
    | B14/0              | fcram_dq_1         |                    | SSTL25_II_BIDI     |
    | B15/1              |                    |                    |                    |
    | B16/1              |                    |                    |                    |
    | B17/1              |                    |                    |                    |
    | B18/1              |                    |                    |                    |
    | B19/1              |                    |                    |                    |
    | B20/1              |                    |                    |                    |
    | B21/1              |                    |                    |                    |
    | B22/1              |                    |                    |                    |
    | C1/7               | ledout_1           |                    | LVCMOS25_OUT       |
    | C4/0               |                    |                    |                    |
    | C5/0               |                    |                    |                    |
    | C6/0               |                    |                    |                    |
    | C7/0               |                    |                    |                    |
    | C8/0               |                    |                    |                    |
    | C9/0               | fcram_addr_3       |                    | SSTL25_II_OUT      |
    | C10/0              | fcram_addr_10      |                    | SSTL25_II_OUT      |
    | C11/0              | fcram_fn           |                    | SSTL25_II_OUT      |
    | C12/0              | fcram_dq_5         |                    | SSTL25_II_BIDI     |
    | C13/0              | vref1B             |                    | LVCMOS12_IN        |
    | C14/1              |                    |                    |                    |
    | C15/1              |                    |                    |                    |
    | C16/1              |                    |                    |                    |
    | C17/1              |                    |                    |                    |
    | C18/1              |                    |                    |                    |
    | C25/2              |                    |                    |                    |
    | C26/2              |                    |                    |                    |
    | D1/7               | ledout_2           |                    | LVCMOS25_OUT       |
    | D2/7               |                    |                    |                    |
    | D4/0               |                    |                    |                    |
    | D6/0               |                    |                    |                    |
    | D7/0               |                    |                    |                    |
    | D8/0               |                    |                    |                    |
    | D9/0               |                    |                    |                    |
    | D10/0              | fcram_addr_0       |                    | SSTL25_II_OUT      |
    | D11/0              | fcram_csn          |                    | SSTL25_II_OUT      |
    | D12/0              | fcram_dq_4         |                    | SSTL25_II_BIDI     |
    | D13/0              | VREF1_BANK_0       |                    |                    |
    | D14/1              | vref2A             |                    | LVCMOS12_IN        |
    | D15/1              |                    |                    |                    |
    | D16/1              |                    |                    |                    |
    | D17/1              |                    |                    |                    |
    | D18/1              |                    |                    |                    |
    | D19/1              |                    |                    |                    |
    | D23/2              |                    |                    |                    |
    | D25/2              |                    |                    |                    |
    | D26/2              |                    |                    |                    |
    | E1/7               | ledout_3           |                    | LVCMOS25_OUT       |
    | E2/7               |                    |                    |                    |
    | E3/7               |                    |                    |                    |
    | E4/7               |                    |                    |                    |
    | E6/0               |                    |                    |                    |
    | E7/0               |                    |                    |                    |
    | E8/0               |                    |                    |                    |
    | E9/0               |                    |                    |                    |
    | E10/0              | fcram_addr_6       |                    | SSTL25_II_OUT      |
    | E11/0              | fcram_addr_9       |                    | SSTL25_II_OUT      |
    | E12/0              | fcram_addr_12      |                    | SSTL25_II_OUT      |
    | E13/1              | vref1A             |                    | LVCMOS12_IN        |
    | E14/1              |                    |                    |                    |
    | E15/1              |                    |                    |                    |
    | E16/1              |                    |                    |                    |
    | E17/1              |                    |                    |                    |
    | E18/1              |                    |                    |                    |
    | E20/1              |                    |                    |                    |
    | E23/2              |                    |                    |                    |
    | F1/7               | ledout_4           |                    | LVCMOS25_OUT       |
    | F2/7               |                    |                    |                    |
    | F3/7               |                    |                    |                    |
    | F6/7               | clk_in             |                    | LVCMOS25_IN        |
    | F7/0               |                    |                    |                    |
    | F8/0               |                    |                    |                    |
    | F9/0               |                    |                    |                    |
    | F10/0              | fcram_addr_5       |                    | SSTL25_II_OUT      |
    | F11/0              | fcram_addr_8       |                    | SSTL25_II_OUT      |
    | F12/0              | fcram_dqs_0        |                    | SSTL25_II_BIDI     |
    | F13/0              | fcram_pdn          |                    | SSTL25_II_OUT      |
    | F14/1              |                    |                    |                    |
    | F15/1              |                    |                    |                    |
    | F16/1              |                    |                    |                    |
    | F17/1              |                    |                    |                    |
    | F18/1              |                    |                    |                    |
    | F19/1              |                    |                    |                    |
    | F21/2              |                    |                    |                    |
    | F25/2              |                    |                    |                    |
    | G1/7               | ledout_5           |                    | LVCMOS25_OUT       |
    | G2/7               |                    |                    |                    |
    | G3/7               |                    |                    |                    |
    | G4/7               |                    |                    |                    |
    | G6/7               |                    |                    |                    |
    | G7/0               |                    |                    |                    |
    | G8/0               |                    |                    |                    |
    | G9/0               |                    |                    |                    |
    | G10/0              | fcram_addr_4       |                    | SSTL25_II_OUT      |
    | G11/0              | fcram_addr_7       |                    | SSTL25_II_OUT      |
    | G12/0              | fcram_addr_11      |                    | SSTL25_II_OUT      |
    | G14/1              |                    |                    |                    |
    | G15/1              |                    |                    |                    |
    | G16/1              |                    |                    |                    |
    | G17/1              |                    |                    |                    |
    | G18/1              |                    |                    |                    |
    | G19/1              |                    |                    |                    |
    | G21/2              |                    |                    |                    |
    | G22/2              |                    |                    |                    |
    | G23/2              |                    |                    |                    |
    | G24/2              |                    |                    |                    |
    | G25/2              |                    |                    |                    |
    | H1/7               | ledout_6           |                    | LVCMOS25_OUT       |
    | H4/7               |                    |                    |                    |
    | H21/2              |                    |                    |                    |
    | H23/2              |                    |                    |                    |
    | H24/2              |                    |                    |                    |
    | H25/2              |                    |                    |                    |
    | H26/2              |                    |                    |                    |
    | J1/7               | ledout_7           |                    | LVCMOS25_OUT       |
    | J4/7               |                    |                    |                    |
    | J5/7               |                    |                    |                    |
    | J6/7               |                    |                    |                    |
    | J20/2              |                    |                    |                    |
    | J24/2              |                    |                    |                    |
    | J25/2              |                    |                    |                    |
    | J26/2              |                    |                    |                    |
    | K1/7               | rst_n              |                    | LVCMOS25_IN        |
    | K2/7               |                    |                    |                    |
    | K3/7               |                    |                    |                    |
    | K4/7               |                    |                    |                    |
    | K5/7               |                    |                    |                    |
    | K6/7               |                    |                    |                    |
    | K20/2              |                    |                    |                    |
    | K21/2              |                    |                    |                    |
    | K22/2              |                    |                    |                    |
    | K23/2              |                    |                    |                    |
    | K24/2              |                    |                    |                    |
    | K25/2              |                    |                    |                    |
    | K26/2              |                    |                    |                    |
    | L1/7               |                    |                    |                    |
    | L2/7               |                    |                    |                    |
    | L3/7               |                    |                    |                    |
    | L4/7               |                    |                    |                    |
    | L5/7               |                    |                    |                    |
    | L6/6               |                    |                    |                    |
    | L7/6               |                    |                    |                    |
    | L21/2              |                    |                    |                    |
    | L22/2              |                    |                    |                    |
    | L23/2              |                    |                    |                    |
    | L24/2              |                    |                    |                    |
    | L25/2              |                    |                    |                    |
    | L26/2              |                    |                    |                    |
    | M1/7               |                    |                    |                    |
    | M2/7               |                    |                    |                    |
    | M3/7               |                    |                    |                    |
    | M4/7               |                    |                    |                    |
    | M5/6               |                    |                    |                    |
    | M6/6               |                    |                    |                    |
    | M21/2              |                    |                    |                    |
    | M22/2              |                    |                    |                    |
    | M23/2              |                    |                    |                    |
    | M24/2              |                    |                    |                    |
    | M25/2              |                    |                    |                    |
    | M26/3              |                    |                    |                    |
    | N1/7               |                    |                    |                    |
    | N2/7               |                    |                    |                    |
    | N4/6               |                    |                    |                    |
    | N5/6               |                    |                    |                    |
    | N6/6               |                    |                    |                    |
    | N21/3              |                    |                    |                    |
    | N22/3              |                    |                    |                    |
    | N23/3              |                    |                    |                    |
    | N24/3              |                    |                    |                    |
    | N25/3              |                    |                    |                    |
    | N26/3              |                    |                    |                    |
    | P1/6               | debug_port_c_15    |                    | LVCMOS25_OUT       |
    | P2/6               | debug_port_c_14    |                    | LVCMOS25_OUT       |
    | P3/6               | debug_port_c_13    |                    | LVCMOS25_OUT       |
    | P4/6               | debug_port_c_12    |                    | LVCMOS25_OUT       |
    | P5/6               | debug_port_c_19    |                    | LVCMOS25_OUT       |
    | P6/6               |                    |                    |                    |
    | P21/3              |                    |                    |                    |
    | P22/3              |                    |                    |                    |
    | P23/3              |                    |                    |                    |
    | P24/3              |                    |                    |                    |
    | P25/3              |                    |                    |                    |
    | P26/3              |                    |                    |                    |
    | R1/6               | debug_port_c_11    |                    | LVCMOS25_OUT       |
    | R2/6               | debug_port_c_10    |                    | LVCMOS25_OUT       |
    | R3/6               | debug_port_c_9     |                    | LVCMOS25_OUT       |
    | R4/6               | debug_port_c_8     |                    | LVCMOS25_OUT       |
    | R5/6               | debug_port_c_18    |                    | LVCMOS25_OUT       |
    | R6/6               |                    |                    |                    |
    | R21/3              |                    |                    |                    |
    | R22/3              |                    |                    |                    |
    | R23/3              |                    |                    |                    |
    | R24/3              |                    |                    |                    |
    | R25/3              |                    |                    |                    |
    | R26/3              |                    |                    |                    |
    | T1/6               | debug_port_c_7     |                    | LVCMOS25_OUT       |
    | T2/6               | debug_port_c_6     |                    | LVCMOS25_OUT       |
    | T3/6               | debug_port_c_5     |                    | LVCMOS25_OUT       |
    | T4/6               | debug_port_c_4     |                    | LVCMOS25_OUT       |
    | T5/6               | debug_port_c_17    |                    | LVCMOS25_OUT       |
    | T6/6               |                    |                    |                    |
    | T21/3              |                    |                    |                    |
    | T22/3              |                    |                    |                    |
    | T23/3              |                    |                    |                    |
    | T24/3              |                    |                    |                    |
    | T25/3              |                    |                    |                    |
    | T26/3              |                    |                    |                    |
    | TCK/6              |                    |                    |                    |
    | TDI/6              |                    |                    |                    |
    | TDO/6              |                    |                    |                    |
    | TMS/6              |                    |                    |                    |
    | U1/6               | debug_port_c_3     |                    | LVCMOS25_OUT       |
    | U2/6               | debug_port_c_2     |                    | LVCMOS25_OUT       |
    | U3/6               | debug_port_c_1     |                    | LVCMOS25_OUT       |
    | U4/6               | debug_port_c_0     |                    | LVCMOS25_OUT       |
    | U5/6               | debug_port_c_16    |                    | LVCMOS25_OUT       |
    | U21/3              |                    |                    |                    |
    | U22/3              |                    |                    |                    |
    | U23/3              |                    |                    |                    |
    | U24/3              |                    |                    |                    |
    | U25/3              |                    |                    |                    |
    | U26/3              |                    |                    |                    |
    | V1/6               |                    |                    |                    |
    | V2/6               |                    |                    |                    |
    | V6/6               |                    |                    |                    |
    | V26/3              |                    |                    |                    |
    | W1/6               |                    |                    |                    |
    | W2/6               |                    |                    |                    |
    | W3/6               |                    |                    |                    |
    | W4/6               |                    |                    |                    |
    | W6/6               |                    |                    |                    |
    | W21/3              |                    |                    |                    |
    | W22/3              |                    |                    |                    |
    | W23/3              |                    |                    |                    |
    | W24/3              |                    |                    |                    |
    | W25/3              |                    |                    |                    |
    | W26/3              |                    |                    |                    |
    | Y1/6               |                    |                    |                    |
    | Y2/6               |                    |                    |                    |
    | Y3/6               |                    |                    |                    |
    | Y4/6               |                    |                    |                    |
    | Y8/5               |                    |                    |                    |
    | Y9/5               |                    |                    |                    |
    | Y10/5              |                    |                    |                    |
    | Y11/5              |                    |                    |                    |
    | Y12/5              |                    |                    |                    |
    | Y14/4              |                    |                    |                    |
    | Y15/4              |                    |                    |                    |
    | Y16/4              |                    |                    |                    |
    | Y17/4              |                    |                    |                    |
    | Y18/4              |                    |                    |                    |
    | Y25/3              |                    |                    | PROHIBITED         |
    | Y26/3              |                    |                    | PROHIBITED         |
    +--------------------+--------------------+--------------------+--------------------+

    sysCONFIG Pins:
      ~ Config_Mode: SLAVE_SERIAL
      ~ Persistent : OFF
    +--------------------+--------------------+--------------------+--------------------+
    |  Pad Name          | sysCONFIG Pin Name |  Pin/Bank          |  Buffer Type       |
    +--------------------+--------------------+--------------------+--------------------+
    | PR42B              | DI                 | Y25/4              |                    |
    | PR42A              | DOUT,CSON          | Y26/4              |                    |
    +--------------------+--------------------+--------------------+--------------------+

    Locate Preferences for each Pin:

    LOCATE  COMP  "clk_in"  SITE  "F6";
    LOCATE  COMP  "debug_port_a_0"  SITE  "AE4";
    LOCATE  COMP  "debug_port_a_1"  SITE  "AE5";
    LOCATE  COMP  "debug_port_a_10"  SITE  "AD7";
    LOCATE  COMP  "debug_port_a_11"  SITE  "AD8";
    LOCATE  COMP  "debug_port_a_12"  SITE  "AD9";
    LOCATE  COMP  "debug_port_a_13"  SITE  "AD10";
    LOCATE  COMP  "debug_port_a_14"  SITE  "AD11";
    LOCATE  COMP  "debug_port_a_15"  SITE  "AD12";
    LOCATE  COMP  "debug_port_a_2"  SITE  "AE6";
    LOCATE  COMP  "debug_port_a_3"  SITE  "AE7";
    LOCATE  COMP  "debug_port_a_4"  SITE  "AE8";
    LOCATE  COMP  "debug_port_a_5"  SITE  "AE9";
    LOCATE  COMP  "debug_port_a_6"  SITE  "AE10";
    LOCATE  COMP  "debug_port_a_7"  SITE  "AD4";
    LOCATE  COMP  "debug_port_a_8"  SITE  "AD5";
    LOCATE  COMP  "debug_port_a_9"  SITE  "AD6";
    LOCATE  COMP  "debug_port_b_0"  SITE  "AF4";
    LOCATE  COMP  "debug_port_b_1"  SITE  "AF5";
    LOCATE  COMP  "debug_port_b_10"  SITE  "AC6";
    LOCATE  COMP  "debug_port_b_11"  SITE  "AC7";
    LOCATE  COMP  "debug_port_b_12"  SITE  "AC8";
    LOCATE  COMP  "debug_port_b_13"  SITE  "AC9";
    LOCATE  COMP  "debug_port_b_14"  SITE  "AC10";
    LOCATE  COMP  "debug_port_b_15"  SITE  "AC11";
    LOCATE  COMP  "debug_port_b_2"  SITE  "AF6";
    LOCATE  COMP  "debug_port_b_3"  SITE  "AF7";
    LOCATE  COMP  "debug_port_b_4"  SITE  "AF8";
    LOCATE  COMP  "debug_port_b_5"  SITE  "AF9";
    LOCATE  COMP  "debug_port_b_6"  SITE  "AF10";
    LOCATE  COMP  "debug_port_b_7"  SITE  "AF11";
    LOCATE  COMP  "debug_port_b_8"  SITE  "AC4";
    LOCATE  COMP  "debug_port_b_9"  SITE  "AC5";
    LOCATE  COMP  "debug_port_c_0"  SITE  "U4";
    LOCATE  COMP  "debug_port_c_1"  SITE  "U3";
    LOCATE  COMP  "debug_port_c_10"  SITE  "R2";
    LOCATE  COMP  "debug_port_c_11"  SITE  "R1";
    LOCATE  COMP  "debug_port_c_12"  SITE  "P4";
    LOCATE  COMP  "debug_port_c_13"  SITE  "P3";
    LOCATE  COMP  "debug_port_c_14"  SITE  "P2";
    LOCATE  COMP  "debug_port_c_15"  SITE  "P1";
    LOCATE  COMP  "debug_port_c_16"  SITE  "U5";
    LOCATE  COMP  "debug_port_c_17"  SITE  "T5";
    LOCATE  COMP  "debug_port_c_18"  SITE  "R5";
    LOCATE  COMP  "debug_port_c_19"  SITE  "P5";
    LOCATE  COMP  "debug_port_c_2"  SITE  "U2";
    LOCATE  COMP  "debug_port_c_3"  SITE  "U1";
    LOCATE  COMP  "debug_port_c_4"  SITE  "T4";
    LOCATE  COMP  "debug_port_c_5"  SITE  "T3";
    LOCATE  COMP  "debug_port_c_6"  SITE  "T2";
    LOCATE  COMP  "debug_port_c_7"  SITE  "T1";
    LOCATE  COMP  "debug_port_c_8"  SITE  "R4";
    LOCATE  COMP  "debug_port_c_9"  SITE  "R3";
    LOCATE  COMP  "fcram_addr_0"  SITE  "D10";
    LOCATE  COMP  "fcram_addr_1"  SITE  "A9";
    LOCATE  COMP  "fcram_addr_10"  SITE  "C10";
    LOCATE  COMP  "fcram_addr_11"  SITE  "G12";
    LOCATE  COMP  "fcram_addr_12"  SITE  "E12";
    LOCATE  COMP  "fcram_addr_13"  SITE  "B11";
    LOCATE  COMP  "fcram_addr_14"  SITE  "A11";
    LOCATE  COMP  "fcram_addr_2"  SITE  "B9";
    LOCATE  COMP  "fcram_addr_3"  SITE  "C9";
    LOCATE  COMP  "fcram_addr_4"  SITE  "G10";
    LOCATE  COMP  "fcram_addr_5"  SITE  "F10";
    LOCATE  COMP  "fcram_addr_6"  SITE  "E10";
    LOCATE  COMP  "fcram_addr_7"  SITE  "G11";
    LOCATE  COMP  "fcram_addr_8"  SITE  "F11";
    LOCATE  COMP  "fcram_addr_9"  SITE  "E11";
    LOCATE  COMP  "fcram_ba_0"  SITE  "A10";
    LOCATE  COMP  "fcram_ba_1"  SITE  "B10";
    LOCATE  COMP  "fcram_clk"  SITE  "A2";
    LOCATE  COMP  "fcram_clkn"  SITE  "A3";
    LOCATE  COMP  "fcram_csn"  SITE  "D11";
    LOCATE  COMP  "fcram_dq_0"  SITE  "A14";
    LOCATE  COMP  "fcram_dq_1"  SITE  "B14";
    LOCATE  COMP  "fcram_dq_2"  SITE  "A13";
    LOCATE  COMP  "fcram_dq_3"  SITE  "B13";
    LOCATE  COMP  "fcram_dq_4"  SITE  "D12";
    LOCATE  COMP  "fcram_dq_5"  SITE  "C12";
    LOCATE  COMP  "fcram_dq_6"  SITE  "A12";
    LOCATE  COMP  "fcram_dq_7"  SITE  "B12";
    LOCATE  COMP  "fcram_dqs_0"  SITE  "F12";
    LOCATE  COMP  "fcram_fn"  SITE  "C11";
    LOCATE  COMP  "fcram_pdn"  SITE  "F13";
    LOCATE  COMP  "ledout_0"  SITE  "B1";
    LOCATE  COMP  "ledout_1"  SITE  "C1";
    LOCATE  COMP  "ledout_2"  SITE  "D1";
    LOCATE  COMP  "ledout_3"  SITE  "E1";
    LOCATE  COMP  "ledout_4"  SITE  "F1";
    LOCATE  COMP  "ledout_5"  SITE  "G1";
    LOCATE  COMP  "ledout_6"  SITE  "H1";
    LOCATE  COMP  "ledout_7"  SITE  "J1";
    LOCATE  COMP  "rst_n"  SITE  "K1";
    LOCATE  COMP  "vref1A"  SITE  "E13";
    LOCATE  COMP  "vref1B"  SITE  "C13";
    LOCATE  COMP  "vref2A"  SITE  "D14";
    LOCATE  COMP  "vref2B"  SITE  "AF3";

    #DQSDLL
    LOCATE  COMP  "U1_fcram_top/ddr_io_u/dqsdll_0"  SITE  "TDLL" ;
    #PLL
    LOCATE  COMP  "U1_fcram_top/sys_clk_pll/ehxpllb_5"  SITE  "PLL3_R40C1" ;

    LOCATE  VREF  "VREF1_BANK_0"  SITE  "D13"  LEVELMODE  "SSTL25_II_BIDI";

    PAR: Place And Route ispLever_v50_Production_Build (40).
    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
    Copyright (c) 1995 AT&T Corp.   All rights reserved.
    Copyright (c) 1995-2001 Lucent Technologies Inc.  All rights reserved.
    Copyright (c) 2001 Agere Systems   All rights reserved.
    Copyright (c) 2002-2005 Lattice Semiconductor Corporation,  All rights reserved.
    Wed Jun 29 14:21:51 2005

    Generated from the file 'C:\EVALUATION BOARDS\EC\HIGH_END\EVAL_CODE\FCRAM\VERILOG\PNR\fcram_verilog_pnr.pad'